   <connector id="connector%3" name="%1.%2" type="female">
      <description>perfboard socket</description>
      <views>
        <breadboardView>
          <p layer="breadboardbreadboard" svgId="connector%3pin"/>
        </breadboardView>
        <schematicView>
          <p layer="breadboardbreadboard" svgId="connector%3pin"/>
        </schematicView>
        <pcbView>
          <p layer="breadboardbreadboard" svgId="connector%3pin"/>
        </pcbView>
      </views>
    </connector>
